**;Load 1A, 2B, 3C, 4D, 5E, 6F and 7A to the accumulator, register B, C, D, E, H and L respectively. Examine the content of each register before and after the execution of each instruction. (Use MVI instruction)**

**MVI A,1AH**

**MVI B,2BH**

**MVI C,3CH**

**MVI D,4DH**

**MVI E,5EH**

**MVI H,6FH**

**MVI L,7AH**

**HLT**