**;Load AABB, CCDD and EEFF into register pair BC, DE and HL respectively. Examine the content of each register before and after the execution of each instruction. (Use LXI instruction)**

**LXI B,0AABBH**

**LXI D,0CCDDH**

**LXI H,0EEFFH**

**HLT**