**;The data 44H and 66H are stored in memory location 9000H and 9001H respectively. Write a program to transfer these data to memory location 9050H and 9051H respectively, use LHLD and SHLD instructions.**

**MVI A,44H**

**STA 9000H**

**MVI A,66H**

**STA 9001H**

**LHLD 9000H**

**SHLD 9050H**

**HLT**