**;Suppose the accumulator content is 25H and register B has 48H. Write a program to subtract the reg B from accumulator and store the result in reg C. Again swap the acc content and reg B content and subtract the reg B content from acc content. See the flag content and the reg content before and after the subtraction**

**MVI A, 25H**

**MVI B, 48H**

**SUB B**

**MOV C,A**

**MOV A,B**

**MOV B,C**

**SUB B**

**HLT**