**;The table along side shows BCD data. Write a program to add the content at memory locations 818A and 818B. Store the BCD result at memory location 818C.**

**MVI A,29**

**MVI B,45**

**ADD B**

**DAA**

**STA 818CH**

**HLT**