**;Write a program to Add the 16-bit BCD data at memory location 8284 with the 16-bit BCD data at 8286 and store the BCD result at 8288.**

**MVI H,13**

**MVI L,79**

**MVI D,26**

**MVI E,48**

**DAD D**

**MOV A,L**

**DAA**

**STA 8288H**

**MOV A,H**

**DAA**

**STA 8289H**

**HLT**