**;Suppose reg H has 34 and reg D has 12. Write program to subtract BCD value in reg D from the BCD value in reg H. Store the BCD result in reg H.**

**MVI H,34**

**MVI D,12**

**MOV A,H**

**SUB D**

**DAA**

**MOV H,A**

**HLT**