**;The content of the memory is shown in the figure along side. Write a program to OR the content of memory location 9024 with the memory location 9025 and store the result at 9026.**

**MVI A,0A2H**

**MVI B,79H**

**ANA B**

**STA 9026H**

**HLT**