**;The content of the memory is shown in the figure along side. Write a program to OR the content of memory location 9024 with the memory location 9025 and store the result at 9026.**

**MVI A,4BH**

**MVI B,0C4H**

**XRA B**

**STA 9029H**

**HLT**