**;Logical instructions can also be used to mask certain bits of a word. Write a program to complement bit D6 of data at memory location 9025. Assume data as shown in the above figure.**

**MVI B,79H**

**MVI A,40H ;D6**

**XRA B**

**STA 9025H**

**HLT**