**;We can complement the accumulator content by using instruction other than CMA How is that possible? Write a program to illustrate this.**

**MVI A,0A7H ; Say A has 0A7H initially**

**CMA**

**STA 0000H ; To Check**

**; Method 1**

**MVI A,0A7H ; Valu of A is repalced by CMA**

**MOV B,A ;B=A**

**MVI A,0FFH ;For A = FF**

**SUB B ; A = FF - B (Initial A)**

**STA 0001H ; Check in Location 0000H & 0001H**

**;Method 2**

**MVI A,0A7H**

**XRI 0FFH**

**STA 0002H ;Check in Location 0000H & 0001H & 0002H**

**HLT**