**;Write a program to set auxiliary flag and reset parity flag without affecting other flags.**

**MVI A,01H**

**ADI 10H ;Set P flag**

**MVI A,08H ;Set AC & Reset P Flag**

**ADI 08H**

**HLT**