**;Write a program to transfer the data at 8020 to 8030 if the data is greater than 127. You can assume data yourself.**

**MVI A,08FH ;Put your number here**

**STA 8020H**

**STC**

**CMC**

**LHLD 8020H**

**CPI 7FH**

**JNC L1**

**HLT**

**L1: JNZ L2**

**HLT**

**L2: STA 8030H**

**HLT**