**;Write a program to copy content of memory location at 8080 to 8090.**

**MVI H,80H**

**MVI L,80H**

**MVI M,0AAH**

**LDA 8080H**

**STA 8090H**

**HLT**