**;Write a program to AND the content of reg B and content of memory at 9030. Assume the content of 9030 as 34 and reg B as 92.**

**MVI B,92H**

**MVI A,34H**

**STA 9030H**

**ANA B**

**HLT**